# `otopcua-modbus-cli` — Modbus-TCP test client

Ad-hoc probe / read / write / subscribe tool for talking to Modbus-TCP devices
through the **same** `ModbusDriver` the OtOpcUa server uses. Mirrors the v1
OPC UA `otopcua-cli` shape so the muscle memory carries over: drop to a shell,
point at a PLC, watch registers move.

First of four driver test-client CLIs (Modbus → AB CIP → AB Legacy → S7 →
TwinCAT). Built on the shared `ZB.MOM.WW.OtOpcUa.Driver.Cli.Common` library
so each downstream CLI inherits verbose/log wiring + snapshot formatting
without copy-paste.

## Build + run

```powershell
dotnet build src/ZB.MOM.WW.OtOpcUa.Driver.Modbus.Cli
dotnet run --project src/ZB.MOM.WW.OtOpcUa.Driver.Modbus.Cli -- --help
```

Or publish a self-contained binary:

```powershell
dotnet publish src/ZB.MOM.WW.OtOpcUa.Driver.Modbus.Cli -c Release -o publish/modbus-cli
publish/modbus-cli/otopcua-modbus-cli.exe --help
```

## Common flags

Every command accepts:

| Flag | Default | Purpose |
|---|---|---|
| `-h` / `--host` | **required** | Modbus-TCP server hostname or IP |
| `-p` / `--port` | `502` | TCP port |
| `-U` / `--unit-id` | `1` | Modbus unit / slave ID |
| `--timeout-ms` | `2000` | Per-PDU timeout |
| `--disable-reconnect` | off | Turn off mid-transaction reconnect-and-retry |
| `--verbose` | off | Serilog debug output |

## Commands

### `probe` — is the PLC up?

Connects, reads one holding register, prints driver health. Fastest sanity
check after swapping a network cable or deploying a new device.

```powershell
otopcua-modbus-cli probe -h 192.168.1.10
otopcua-modbus-cli probe -h 192.168.1.10 --probe-address 100    # device locks HR[0]
```

### `read` — single register / coil / string

Synthesises a one-tag driver config on the fly from `--region` + `--address`
+ `--type` flags.

```powershell
# Holding register as UInt16
otopcua-modbus-cli read -h 192.168.1.10 -r HoldingRegisters -a 100 -t UInt16

# Float32 with word-swap (CDAB) — common on Siemens / some AB families
otopcua-modbus-cli read -h 192.168.1.10 -r HoldingRegisters -a 200 -t Float32 --byte-order WordSwap

# Single bit out of a packed holding register
otopcua-modbus-cli read -h 192.168.1.10 -r HoldingRegisters -a 10 -t BitInRegister --bit-index 3

# 40-char ASCII string — DirectLOGIC packs the first char in the low byte
otopcua-modbus-cli read -h 192.168.1.10 -r HoldingRegisters -a 300 -t String --string-length 40 --string-byte-order LowByteFirst

# Discrete input / coil
otopcua-modbus-cli read -h 192.168.1.10 -r DiscreteInputs -a 5 -t Bool
```

### `write` — single value

Same flag shape as `read` plus `-v` / `--value`. Values parse per `--type`
using invariant culture (period as decimal separator). Booleans accept
`true`/`false`/`1`/`0`/`yes`/`no`/`on`/`off`.

```powershell
otopcua-modbus-cli write -h 192.168.1.10 -r HoldingRegisters -a 100 -t UInt16 -v 42
otopcua-modbus-cli write -h 192.168.1.10 -r HoldingRegisters -a 200 -t Float32 -v 3.14
otopcua-modbus-cli write -h 192.168.1.10 -r Coils -a 5 -t Bool -v on
```

**Writes are non-idempotent by default** — a timeout after the device
already applied the write will NOT auto-retry. This matches the driver's
production contract (plan decisions #44 + #45).

### `subscribe` — watch a register until Ctrl+C

Uses the driver's `ISubscribable` surface (polling under the hood via
`PollGroupEngine`). Prints every data-change event with a timestamp.

```powershell
otopcua-modbus-cli subscribe -h 192.168.1.10 -r HoldingRegisters -a 100 -t Int16 -i 500
```

## Output format

- `probe` / `read` emit a multi-line per-tag block: `Tag / Value / Status /
  Source Time / Server Time`.
- `write` emits one line: `Write <tag>: 0x... (Good | BadCommunicationError | …)`.
- `subscribe` emits one line per change: `[HH:mm:ss.fff] <tag> = <value> (<status>)`.

Status codes are rendered as `0xXXXXXXXX (Name)` for the OPC UA shortlist
(`Good`, `BadCommunicationError`, `BadTimeout`, `BadNodeIdUnknown`,
`BadTypeMismatch`, `Uncertain`, …). Unknown codes fall back to bare hex.

## Typical workflows

**"Is the PLC alive?"** → `probe`.

**"Does my recipe write land?"** → `write` + `read` back against the same
address.

**"Why is tag X flipping?"** → `subscribe` + wait for the operator scenario.

**"What's the right byte order for this family?"** → `read` with
`--byte-order BigEndian`, then with `--byte-order WordSwap`. The one that
gives plausible values is the correct one for that device.
