# Read/Write Operations

The v2 server routes OPC UA Read and Write operations to each driver's `IReadable` and `IWritable` capabilities through `CapabilityInvoker` so the Polly pipeline (retry / timeout / breaker) applies uniformly across Galaxy, Modbus, S7, AB CIP, AB Legacy, TwinCAT, FOCAS, and OPC UA Client drivers. The per-variable `OnReadValue` and `OnWriteValue` hooks described in the sections below live in `DriverNodeManager` (the planned ADR-002 Phase 7 Stream G successor to the v1 `DriverNodeManager`); `GenericDriverNodeManager` (`src/Core/ZB.MOM.WW.OtOpcUa.Core/OpcUa/GenericDriverNodeManager.cs`) handles address-space population and alarm routing during discovery. The current `OtOpcUaNodeManager` (`src/Server/ZB.MOM.WW.OtOpcUa.OpcUaServer/OtOpcUaNodeManager.cs`) is a push-model `CustomNodeManager2` that receives values from the Akka actor layer via `WriteValue`; OPC UA client reads return the cached pushed value.

## Driver vs virtual dispatch

Per [ADR-002](v2/implementation/adr-002-driver-vs-virtual-dispatch.md), a single `DriverNodeManager` routes reads and writes across both driver-sourced and virtual (scripted) tags. At discovery time each variable registers a `NodeSourceKind` (`src/Core/ZB.MOM.WW.OtOpcUa.Core.Abstractions/DriverAttributeInfo.cs`) in the manager's `_sourceByFullRef` lookup; the read/write hooks pattern-match on that value to pick the backend:

- `NodeSourceKind.Driver` — dispatches to the driver's `IReadable` / `IWritable` through `CapabilityInvoker` (the rest of this doc).
- `NodeSourceKind.Virtual` — dispatches to `VirtualTagSource` (`src/Core/ZB.MOM.WW.OtOpcUa.Core.VirtualTags/VirtualTagSource.cs`), which wraps `VirtualTagEngine`. Writes are rejected with `BadUserAccessDenied` before the branch per Phase 7 decision #6 — scripts are the only write path into virtual tags.
- `NodeSourceKind.ScriptedAlarm` — dispatches to the Phase 7 `ScriptedAlarmReadable` shim.

ACL enforcement (`WriteAuthzPolicy` + `AuthorizationGate`) runs before the source branch, so the gates below apply uniformly to all three source kinds.

## OnReadValue

The hook is registered on every `BaseDataVariableState` created by the `IAddressSpaceBuilder.Variable(...)` call during discovery. When the stack dispatches a Read for a node in this namespace:

1. If the driver does not implement `IReadable`, the hook returns `BadNotReadable`.
2. The node's `NodeId.Identifier` is used directly as the driver-side full reference — it matches `DriverAttributeInfo.FullName` registered at discovery time.
3. (Phase 6.2) If an `AuthorizationGate` + `NodeScopeResolver` are wired, the gate is consulted first via `IsAllowed(identity, OpcUaOperation.Read, scope)`. A denied read never hits the driver.
4. The call is wrapped by `_invoker.ExecuteAsync(DriverCapability.Read, ResolveHostFor(fullRef), …)`. The resolved host is `IPerCallHostResolver.ResolveHost(fullRef)` for multi-host drivers; single-host drivers fall back to `DriverInstanceId` (decision #144).
5. The first `DataValueSnapshot` from the batch populates the outgoing `value` / `statusCode` / `timestamp`. An empty batch surfaces `BadNoData`; any exception surfaces `BadInternalError`.

The hook is synchronous — the async invoker call is bridged with `AsTask().GetAwaiter().GetResult()` because the OPC UA SDK's value-hook signature is sync. Idempotent-by-construction reads mean this bridge is safe to retry inside the Polly pipeline.

## OnWriteValue

`OnWriteValue` follows the same shape with two additional concerns: authorization and idempotence.

### Authorization (two layers)

1. **SecurityClassification gate.** Every variable stores its `SecurityClassification` in `_securityByFullRef` at registration time (populated from `DriverAttributeInfo.SecurityClass`). `WriteAuthzPolicy.IsAllowed(classification, userRoles)` runs first, consulting the session's roles via `context.UserIdentity is IRoleBearer`. `FreeAccess` passes anonymously, `ViewOnly` denies everyone, and `Operate / Tune / Configure / SecuredWrite / VerifiedWrite` require `WriteOperate / WriteTune / WriteConfigure` roles respectively. Denial returns `BadUserAccessDenied` without consulting the driver — drivers never enforce ACLs themselves; they only report classification as discovery metadata (see `docs/security.md`).
2. **Phase 6.2 permission-trie gate.** When `AuthorizationGate` is wired, it re-runs with the operation derived from `WriteAuthzPolicy.ToOpcUaOperation(classification)`. The gate consults the per-cluster permission trie loaded from `NodeAcl` rows, enforcing fine-grained per-tag ACLs on top of the role-based classification policy. See `docs/v2/acl-design.md`.

### Dispatch

`_invoker.ExecuteWriteAsync(host, isIdempotent, callSite, …)` honors the `WriteIdempotentAttribute` semantics per decisions #44-45 and #143:

- `isIdempotent = true` (tag flagged `WriteIdempotent` in the Config DB) → runs through the standard `DriverCapability.Write` pipeline; retry may apply per the tier configuration.
- `isIdempotent = false` (default) → the invoker builds a one-off pipeline with `RetryCount = 0`. A timeout may fire after the device already accepted the pulse / alarm-ack / counter-increment; replay is the caller's decision, not the server's.

The `_writeIdempotentByFullRef` lookup is populated at discovery time from the `DriverAttributeInfo.WriteIdempotent` field.

### Per-write status

`IWritable.WriteAsync` returns `IReadOnlyList<WriteResult>` — one numeric `StatusCode` per requested write. A non-zero code is surfaced directly to the client; exceptions become `BadInternalError`. The OPC UA stack's pattern of batching per-service is preserved through the full chain.

## Array element writes

Array-element writes via OPC UA `IndexRange` are driver-specific. The OPC UA stack hands the dispatch an unwrapped `NumericRange` on the `indexRange` parameter of `OnWriteValue`; `DriverNodeManager` passes the full `value` object to `IWritable.WriteAsync` and the driver decides whether to support partial writes. Galaxy performs a read-modify-write inside the Galaxy driver (MXAccess has no element-level writes); other drivers generally accept only full-array writes today.

## HistoryRead

`DriverNodeManager.HistoryReadRawModified`, `HistoryReadProcessed`, `HistoryReadAtTime`, and `HistoryReadEvents` route through the driver's `IHistoryProvider` capability with `DriverCapability.HistoryRead`. Drivers without `IHistoryProvider` surface `BadHistoryOperationUnsupported` per node. See `docs/v1/HistoricalDataAccess.md`.

## Failure isolation

Per decision #12, exceptions in the driver's capability call are logged and converted to a per-node `BadInternalError` — they never unwind into the master node manager. This keeps one driver's outage from disrupting sibling drivers in the same server process.

## Key source files

- `src/Core/ZB.MOM.WW.OtOpcUa.Core/OpcUa/GenericDriverNodeManager.cs` — address-space population and alarm routing during discovery
- `src/Server/ZB.MOM.WW.OtOpcUa.OpcUaServer/OtOpcUaNodeManager.cs` — push-model `CustomNodeManager2`; `EnsureVariable` / `WriteValue` are the v2 read/write path
- `src/Core/ZB.MOM.WW.OtOpcUa.Core/Authorization/` — permission trie + evaluator (`PermissionTrie`, `PermissionTrieCache`, `TriePermissionEvaluator`) that gates Read/Write/Subscribe per the session's resolved LDAP groups
- `src/Core/ZB.MOM.WW.OtOpcUa.Core/Resilience/CapabilityInvoker.cs` — `ExecuteAsync` / `ExecuteWriteAsync`
- `src/Core/ZB.MOM.WW.OtOpcUa.Core.Abstractions/IReadable.cs`, `IWritable.cs`, `WriteIdempotentAttribute.cs`
